{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-E6V / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHBH08EF6V / ERGA06EAV3H","EHBH08EA6V / ERGA06EAV3H"]
["Capacidad de calefacción","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Consumo","Calefacción","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 55°C","General","SCOP","","3.26","3.26"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","Clase de efic. estac. de calef. de habitaciones","","A++","A++"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 35°C","General","SCOP","","4.47","4.47"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 35°C","General","Clase de efic. estac. de calef. de habitaciones","","A+++","A+++"]
["Rango de eficiencia energética","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notas","","","","","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)"]