{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHSH08P30EF / ERGA06EAV3H","EHSH08P50EF / ERGA06EAV3H","EHSH08P30EG / ERGA06EAV3H","EHSH08P50EG / ERGA06EAV3H"]
["Unidad interior","","","","","EHSH08P30EF","EHSH08P50EF","EHSH08P30EG","EHSH08P50EG"]
["Capacidad de calefacción","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Consumo","Calefacción","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["Calentamiento de agua caliente sanitaria","General","","Perfil de carga declarado","","L","XL","L","XL"]
["","Clima medio","","Clase de eficiencia energética de calentamiento de agua","","A+","A+","A+","A+"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 55°C","General","SCOP","","3.26","3.26","3.26","3.26"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","Clase de efic. estac. de calef. de habitaciones","","A++","A++","A++","A++"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 35°C","General","SCOP","","4.47","4.47","4.47","4.47"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 35°C","General","Clase de efic. estac. de calef. de habitaciones","","A+++","A+++","A+++","A+++"]
["Notas","","","","","(1) - Condición 1: refrigeración Ta 35°C - LWE 18℃ (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18℃ (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condición 2: refrigeración Ta 35°C - LWE 7℃ (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7℃ (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)"]