{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3 / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3 / ERGA04EAV3"]
["Calentamiento de agua caliente sanitaria","General","","Perfil de carga declarado","","L"]
["","Clima medio","","Clase de eficiencia energética de calentamiento de agua","","A+"]
["COP","","","","","5.10 (1), 3.65 (2)"]
["Unidad interior","","","","","EHSHB04P30DA3"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","Seasonal space heating eff. class","","A++"]
["","","","ηs (Efic. estac. de calef. de habitaciones)","%","127"]
["","","","SCOP","","3.26"]
["Capacidad de calefacción","Nom.","","","kW","4.30 (1), 4.60 (2)"]
["Consumo","Calefacción","","Nom.","kW","0.840 (1), 1.26 (2)"]
["Notas","","","","","(1) - Condición 1: refrigeración Ta 35°C - LWE 18℃ (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condición 2: refrigeración Ta 35°C - LWE 7℃ (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45℃ (DT = 5°C)"]