{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-D3"]
[]
[]
[]
[]
["","","","","","EHSXB04P30DA3"]
["Carcasa","Color","","","","Blanco tráfico (RAL9016) / Gris oscuro (RAL7011)"]
["","Material","","","","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","","Altura","mm","1891"]
["","","","Anchura","mm","595"]
["","","","Profundidad","mm","615"]
["Peso","Unidad","","","kg","76.0"]
["PED","Categoría","","","","art. 3,3"]
["Refrigerante","Tipo","","","","R-32"]
["","GWP","","","","675.0"]
["","Carga","","","kg","1.50"]
["Nivel de potencia sonora","Nom.","","","dBA","39"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","18"]
["","","","Máx.","°C","65"]
["","Refrigeración","Ambiente","Mín.","°CBS","10"]
["","","Lado del agua","Mín.","°C","5"]
["","","","Máx.","°C","22"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","230"]
["Calentador eléctrico","Alimentación eléctrica","","Nombre","","3V / 9W"]
["","","","Fase","","1~ / 3~"]
["","","","Frecuencia","Hz","50"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]