{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E"]
[]
[]
[]
[]
["","","","","","EHSXB04P30EF","EHSXB04P50EF","EHSXB04P30EG","EHSXB04P50EG","EHSXB08P30EF","EHSXB08P50EF","EHSXB08P30EG","EHSXB08P50EG"]
["Carcasa","Color","","","","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)"]
["","Material","","","","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","","Altura","mm","1,892","1,905","1,891","1,910","1,892","1,905","1,891","1,910"]
["","","","Anchura","mm","594","792","594","792","594","792","594","792"]
["","","","Profundidad","mm","644","812","644","817","644","812","644","817"]
["Peso","Unidad","","","kg","79","110","80.0","104","79","110","80.0","104"]
["PED","Categoría","","","","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675","675.0","675.0","675","675","675.0","675.0"]
["","Carga","","","kg","1.5","1.5","1.50","1.50","1.5","1.5","1.50","1.50"]
["Nivel de potencia sonora","Nom.","","","dBA","39","39","39","39","39","39","39","39"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","18","18","18","18","18","18","18","18"]
["","","","Máx.","°C","65","65","65","65","65","65","65","65"]
["","Refrigeración","Ambiente","Mín.","°CBS","10","10","10","10","10","10","10","10"]
["","","Lado del agua","Mín.","°C","5","5","5","5","5","5","5","5"]
["","","","Máx.","°C","22","22","22","22","22","22","22","22"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50","50","50"]
["","Tensión","","","V","230","230","230","230","230","230","230","230"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]