{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E3V / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA3V / ERGA04EAV3","EHVX04S18EJ3V / ERGA04EAV3","EHVX04S23EA3V / ERGA04EAV3","EHVX04S23EJ3V / ERGA04EAV3"]
["Capacidad de calefacción","Nom.","","","kW","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)"]
["Capacidad de refrigeración","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Consumo","Calefacción","","Nom.","kW","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)"]
["","Refrigeración","","Nom.","kW","0.81 (1), 1.36 (2)","0.81 (1), 1.36 (2)","0.81 (1), 1.36 (2)","0.81 (1), 1.36 (2)"]
["","Agua caliente sanitaria de 10°C a 50 °C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Tiempo de calentamiento de 10°C a 50 °C","hr","","","","1h28min","1h28min","1h40min","1h40min"]
["COP","","","","","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Calentamiento de agua caliente sanitaria","General","","Perfil de carga declarado","","L","L","XL","XL"]
["","Clima medio","","Clase de eficiencia energética de calentamiento de agua","","A+","A+","A+","A+"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 55°C","General","SCOP","","3.29","3.29","3.29","3.29"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","Clase de efic. estac. de calef. de habitaciones","","A++","A++","A++","A++"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 35°C","General","SCOP","","4.54","4.54","4.54","4.54"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 35°C","General","Clase de efic. estac. de calef. de habitaciones","","A+++","A+++","A+++","A+++"]
["Notas","","","","","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)"]