{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCB-CV3"]
[]
[]
[]
[]
["","","","","EKCB07CAV3"]
["Dimensiones","Unidad","Anchura","mm","340"]
["","","Profundidad","mm","97.0"]
["","","Altura","mm","360"]
["Carcasa","Material","","","Planchas metálicas revestidas"]
["","Color","","","Blanco"]
["Peso","Unidad","","kg","4.00"]
["Conexiones de cableado","Para conectar la alimentación eléctrica al modelo *KHW* + Q2L","Observación","","sección de cable 2,5 mm2"]
["","","Cantidad","","4 + GND"]
["","Para conexión con interfaz de usuario","Observación","","100 mA, 0,75 mm² hasta 1,25 mm² (longitud máx. 500 m)"]
["","","Cantidad","","2"]
["Power supply","Fase","","","1~"]
["","Frecuencia","","Hz","50"]
["","Tensión","","V","230"]
["Corriente","Fusibles recomendados","","A","10"]
["Notas","","","","(1) - El equipo cumple con la norma EN/IEC 61000-3-12: norma técnica internacional y europea que limita las corrientes armónicas producidas por los equipos conectados al sistema público de baja tensión con una corriente de entrada mayor de 16 A e igual o inferior a 75 A por fase."]
["","","","","(2) - Entre *KCB*C* y *K2CB*C*"]
["","","","","(3) - Seleccione el diámetro y el tipo de acuerdo con los reglamentos vigentes en su país o región."]