{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montaje","","","","","Pared","Pared"]
["Carcasa","Color","","","","Blanco + Negro","Blanco + Negro"]
["","Material","","","","Metal laminado, Acrilonitrilo Butadieno Estireno","Metal laminado, Acrilonitrilo Butadieno Estireno"]
["Dimensiones","Unidad","Altura","Depósito","mm","1032","1283"]
["","","","Anchura","mm","510","510"]
["","","","Profundidad","mm","570","570"]
["Peso","Unidad","","Vacío","kg","43","47"]
["Depósito","Volumen de agua","","","l","89","118"]
["","Material","","","","Acero esmaltado según norma DIN4753TL2","Acero esmaltado según norma DIN4753TL2"]
["","Máxima temperatura del agua","","","°C","75.0","75.0"]
["","Clase de eficiencia energética","","","","B","C"]
["Intercambiador de calor","Agua caliente sanitaria","","Cantidad","","1","1"]
["","","","Material del tubo","","Aluminio","Aluminio"]
["","","","Presión de funcionamiento","bares","42","42"]
["Calentador eléctrico auxiliar","Capacidad","","","kW","1.2","1.2"]