{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-B"]
[]
[]
[]
[]
["","","","","","EKHWP300B","EKHWP54419BA","EKHWP500B"]
["Intercambiador de calor","Agua caliente sanitaria","","Material del tubo","","","Acero inoxidable (DIN 1,4404)"]
["","","","Presión de funcionamiento","bar","","10.0"]
["","","","Volumen interno de la batería","l","","28.9"]
["","","","Cantidad","","","1"]
["","Carga","","Cantidad","","","1"]
["","","","Material del tubo","","","Acero inoxidable (DIN 1,4404)"]
["","","","Presión de funcionamiento","bar","","3.0"]
["","","","Volumen interno de la batería","l","","10.0"]
["","Calefacción solar auxiliar","","Volumen interno de la batería","l","","3.9"]
["","","","Material del tubo","","","Acero inoxidable (DIN 1,4404)"]
["","","","Presión de funcionamiento","bar","","3.0"]
["","","","Cantidad","","","1"]
["Dimensiones","Unidad","","Anchura","mm","","790"]
["","","Altura","Depósito","mm","","1,658"]
["","","","Profundidad","mm","","790"]
["Carcasa","Material","","","","","Polipropileno resistente a impactos"]
["","Colour","","","","","Blanco tráfico (RAL9016) / Gris oscuro (RAL7011)"]
["Depósito","Clase de eficiencia energética","","","","","B"]
["","Máxima temperatura del agua","","","°C","","85"]
["","Material","","","","","Polipropileno"]
["","Volumen de agua","","","l","","477"]
["Peso","Unidad","","Vacío","kg","","71"]
["","","","Total","kg","","548"]
["Montaje","","","","","","Suelo"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]
["","","","","","(5) - Para volumen de aprovechamiento 140l -> 5820 Wh (baño) / 8kW bomba de calor","(5) - Para volumen de aprovechamiento 140l -> 5820 Wh (baño) / 8kW bomba de calor","(5) - Para volumen de aprovechamiento 140l -> 5820 Wh (baño) / 16kW bomba de calor"]
["","","","","","(6) - Para volumen de aprovechamiento 90l -> 3660 Wh (baño) / 8kW bomba de calor","(6) - Para volumen de aprovechamiento 90l -> 3660 Wh (baño) / 8kW bomba de calor","(6) - Para volumen de aprovechamiento 90l -> 3660 Wh (baño) / 16kW bomba de calor"]
["","","","","","","(7) - Para volumen de aprovechamiento 140l -> 5820 Wh (baño) / 16kW bomba de calor"]
["","","","","","","(8) - Para volumen de aprovechamiento 90l -> 3660 Wh (baño) / 16kW bomba de calor"]
["","","","","","","(9) - Intercambiador de calor conectado en paralelo, TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]
["","","","","","","(10) - TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]
["Montaje","","","","","Suelo","","Suelo"]
["Carcasa","Color","","","","Blanco tráfico (RAL9016) / Gris oscuro (RAL7011)","","Blanco tráfico (RAL9016) / Gris oscuro (RAL7011)"]
["","Material","","","","Polipropileno resistente a impactos","","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","Altura","Depósito","mm","1646","","1658"]
["","","","Anchura","mm","595","","790"]
["","","","Profundidad","mm","615","","790"]
["Peso","Unidad","","Vacío","kg","53","","76"]
["","","","Total","kg","347","","553"]
["Depósito","Volumen de agua","","","l","294","","477"]
["","Material","","","","Polipropileno","","Polipropileno"]
["","Máxima temperatura del agua","","","°C","85","","85"]
["","Clase de eficiencia energética","","","","B","","B"]
["Intercambiador de calor","Agua caliente sanitaria","","Cantidad","","1","","1"]
["","","","Material del tubo","","Acero inoxidable (DIN 1.4404)","","Acero inoxidable (DIN 1.4404)"]
["","","","Volumen interno de la batería","l","27.8","","28.9"]
["","","","Presión de funcionamiento","bar","10.0","","10.0"]
["","Carga","","Cantidad","","1","","1"]
["","","","Material del tubo","","Acero inoxidable (DIN 1.4404)","","Acero inoxidable (DIN 1.4404)"]
["","","","Volumen interno de la batería","l","12.9","","18.1"]
["","","","Presión de funcionamiento","bar","6.0","","6.0"]
["","Calefacción solar auxiliar","","Cantidad","","","","1"]
["","","","Material del tubo","","","","Acero inoxidable (DIN 1.4404)"]
["","","","Volumen interno de la batería","l","","","3.9"]
["","","","Presión de funcionamiento","bar","","","3.0"]