{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150D3V3","EKHWS180D3V3","EKHWS200D3V3","EKHWS250D3V3","EKHWS300D3V3"]
["Carcasa","Color","","","","Blanco neutro","Blanco neutro","Blanco neutro","Blanco neutro","Blanco neutro"]
["","Material","","","","Acero recubierto de epoxi, Acero dulce recubierto de epoxi","Acero recubierto de epoxi, Acero dulce recubierto de epoxi","Acero recubierto de epoxi, Acero dulce recubierto de epoxi","Acero recubierto de epoxi, Acero dulce recubierto de epoxi","Acero recubierto de epoxi, Acero dulce recubierto de epoxi"]
["Dimensiones","Unidad","Altura","Depósito","mm","1,000","1,164","1,264","1,535","1,745"]
["","","","Diámetro","mm","595","595","595","595","595"]
["Peso","Unidad","","Vacío","kg","45","50","53","58","63"]
["","","","Total","kg","190","224","245","300","355"]
["Depósito","Volumen de agua","","","l","145","174","192","242","292"]
["","Material","","","","Acero inoxidable (EN 1,4521)","Acero inoxidable (EN 1,4521)","Acero inoxidable (EN 1,4521)","Acero inoxidable (EN 1,4521)","Acero inoxidable (EN 1,4521)"]
["","Máxima temperatura del agua","","","°C","75","75","75","75","75"]
["","Clase de eficiencia energética","","","","B","B","B","B","B"]
["Intercambiador de calor","Agua caliente sanitaria","","Cantidad","","1","1","1","1","1"]
["","","","Material del tubo","","Acero inoxidable (EN 1.4521)","Acero inoxidable (EN 1.4521)","Acero inoxidable (EN 1.4521)","Acero inoxidable (EN 1.4521)","Acero inoxidable (EN 1.4521)"]
["","","","Volumen interno de la batería","l","4.9","6.5","8.2","8.2","8.2"]
["","","","Presión de funcionamiento","bar","10","10","10","10","10"]
["Calentador eléctrico auxiliar","Capacidad","","","kW","3","3","3","3","3"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]