{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P","EKSV21P1","EKSV26P","EKSV26P1"]
["Absorbedor","","","","Registro de tubería de cobre en forma de arpa con placa revestida de aluminio muy selectiva soldada a láser.","Registro de tubería de cobre en forma de arpa con placa revestida de aluminio muy selectiva soldada a láser.","Registro de tubería de cobre en forma de arpa con placa revestida de aluminio muy selectiva soldada a láser.","Registro de tubería de cobre en forma de arpa con placa revestida de aluminio muy selectiva soldada a láser."]
["Temperatura de parada","Máx.","","°C","192","192","192","192"]
["Dimensiones","Unidad","Anchura","mm","85","1,006","85","1,300"]
["","","Profundidad","mm","2,000","85","2,000","85"]
["","","Altura","mm","1,006","2,000","1,300","2,000"]
["Presión de funcionamiento","Máx.","","bar","6","6","6","6"]
["Peso","Unidad","","kg","33","35","42","42"]
["Superficie","Abertura","","m²","1.800","1.800","2.360","2.360"]
["","Absorbedor","","m²","1.79","1.80","2.35","2.36"]
["","Exterior","","m²","2.01","2.01","2.60","2.60"]
["Montaje","","","","Vertical","Vertical","Vertical","Vertical"]
["Acristalado","","","","Vidrio de seguridad del panel sencillo, transmisión +/- 92%","Vidrio de seguridad del panel sencillo, transmisión +/- 92%","Vidrio de seguridad del panel sencillo, transmisión +/- 92%","Vidrio de seguridad del panel sencillo, transmisión +/- 92%"]
["Ángulo de techo permitido","Máx.","","°","80","80","80","80"]
["","Mín.","","°","15","15","15","15"]
["Revestimiento","","","","Micro-therm (máx.absorción 96%, emisión 5% +/-2%)","Micro-therm (máx.absorción 96%, emisión 5% +/-2%)","Micro-therm (máx.absorción 96%, emisión 5% +/-2%)","Micro-therm (máx.absorción 96%, emisión 5% +/-2%)"]
["Volumen","l","","","1.3","1.3","1.7","1.7"]
["Rendimiento térmico","Eficiencia del colector sin pérdidas η0","","%","0.781","0.710","0.784","0.710"]
["","Coeficiente de pérdida de calor a1","","W/m².K","4.240","4.300","4.250","4.300"]
["","Dependencia de temperatura  del coeficiente de pérdida de calor a2","","W/m².K²","0.006","0.006","0.007","0.006"]
["","Capacidad térmica","","kJ/K","4.9","4.9","6.5","6.5"]