{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSXB-E"]
[]
[]
[]
[]
["","","","","","ELSXB12P30EG","ELSXB12P50EG","ELSXB12P30EF (Archived)","ELSXB12P50EF (Archived)"]
["Carcasa","Color","","","","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)"]
["","Material","","","","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","","Altura","mm","1891","1910","1893","1910"]
["","","","Anchura","mm","594","792","594","792"]
["","","","Profundidad","mm","680","817","680","817"]
["Peso","Unidad","","","kg","93.0","115","76.0","91.0"]
["PED","Categoría","","","","Categoría II","Categoría II","Categoría II","Categoría II"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32"]
["Nivel de potencia sonora","Nom.","","","dBA","44.7","44.7","44.7","44.7"]
["Nivel de presión sonora","Nom.","","","dBA","36.8","36.8","36.8","36.8"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Máx.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Refrigeración","Ambiente","Mín.","°CBS","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Lado del agua","Mín.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Máx.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50"]
["","Tensión","","","V","230","230","230","230"]
["Notas","","","","","(1) - El área de funcionamiento se amplía a caudales más bajos dependiendo del modo de funcionamiento: consulte la curva ESP.","(1) - El área de funcionamiento se amplía a caudales más bajos dependiendo del modo de funcionamiento: consulte la curva ESP.","(1) - El área de funcionamiento se amplía a caudales más bajos dependiendo del modo de funcionamiento: consulte la curva ESP.","(1) - El área de funcionamiento se amplía a caudales más bajos dependiendo del modo de funcionamiento: consulte la curva ESP."]
["","","","","","(2) - Pérdida de calor conforme a EN12897","(2) - Pérdida de calor conforme a EN12897","(2) - Pérdida de calor conforme a EN12897","(2) - Pérdida de calor conforme a EN12897"]
["","","","","","(3) - Encontrará más detalles en el diagrama de límites de funcionamiento.","(3) - Encontrará más detalles en el diagrama de límites de funcionamiento.","(3) - Encontrará más detalles en el diagrama de límites de funcionamiento.","(3) - Encontrará más detalles en el diagrama de límites de funcionamiento."]