{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK12-14AW1"]
[]
[]
[]
[]
["","","","","","EPSK12ARW1","EPSK14ARW1"]
["Dimensiones","Unidad","","Altura","mm","1,123","1,123"]
["","","","Anchura","mm","1,330","1,330"]
["","","","Profundidad","mm","604","604"]
["Peso","Unidad","","","kg","191","191"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","96.3","96.3"]
["","","Refrigeración","Alto","m³/min","96.3","96.3"]
["Límites de func.","Refrigeración","","Mín.","°CBS","10","10"]
["","","","Máx.","°CBS","43","43"]
["Límites de funcionamiento","Agua caliente sanitaria","","Mín.","°CBS","-28","-28"]
["Límites de func.","Límites de func.-=-Agua caliente sanitaria","","Máx.","°CBS","40","40"]
["Nivel de potencia sonora","Calefacción","","Nom.","dBA","52 (1)","52 (1)"]
["","Refrigeración","","Nom.","dBA","62 (2)","63 (2)"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","38 (1)","38 (1)"]
["","Refrigeración","","Nom.","dBA","47 (2)","48 (2)"]
["Refrigerante","Tipo","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["","Carga","","","tCO2Eq","0.0038","0.0038"]
["","Carga","","","kg","1.25","1.25"]
["Conexiones de tubería","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","10","10"]
["Alimentación eléctrica","Nombre","","","","W1","W1"]
["","Fase","","","","3~","3~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","400","400"]
["Corriente","Fusibles recomendados","","","A","16","16"]
["Notas","","","","","(1) - Medido a una LWC 47-55 °C ; Ta BS/BH 7 °C/ 6 °C.","(1) - Medido a una LWC 47-55 °C ; Ta BS/BH 7 °C/ 6 °C."]
["","","","","","(2) - Medido a una LWC 12-7 °C ; Ta 35 °C.","(2) - Medido a una LWC 12-7 °C ; Ta 35 °C."]
["","","","","","(3) - Tubería en la obra 1 1/4\"","(3) - Tubería en la obra 1 1/4\""]
["","","","","","(4) - Tubería en la obra 1 1/2\"","(4) - Tubería en la obra 1 1/2\""]