{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB14A"]
[]
[]
[]
[]
["","","","","","EPSXB14P30AF","EPSXB14P50AF"]
["Carcasa","Color","","","","Blanco tráfico (RAL9016), Negro grafito (RAL9011), Negro Jet (RAL9005)","Blanco tráfico (RAL9016), Negro grafito (RAL9011), Negro Jet (RAL9005)"]
["","Material","","","","Polipropileno resistente a impactos","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","","Altura","mm","1914","1906"]
["","","","Anchura","mm","590","785"]
["","","","Profundidad","mm","671","837"]
["Peso","Unidad","","","kg","87.0","109"]
["PED","Categoría","","","","Art. 4.3","Art. 4.3"]
["Nivel de potencia sonora","Nom.","","","dBA","49.0","49.0"]
["Nivel de presión sonora","Nom.","","","dBA","35.0","35.0"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","0 (3)","0 (3)"]
["","","","Máx.","°C","0 (3)","0 (3)"]
["","Refrigeración","Ambiente","Mín.","°CBS","0 (3)","0 (3)"]
["","","Lado del agua","Mín.","°C","0 (3)","0 (3)"]
["","","","Máx.","°C","0 (3)","0 (3)"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","230","230"]
["Calentador eléctrico","Alimentación eléctrica","","Nombre","","6V / 9W","6V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["","","","Frecuencia","Hz","50","50"]
["","","","Tensión","V","230/400","230/400"]
["","Fusibles recomendados","","","A","0 (4)","0 (4)"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]
["","","","","","(2) - Volumen mínimo necesario, excluyendo el volumen de la unidad","(2) - Volumen mínimo necesario, excluyendo el volumen de la unidad"]
["","","","","","(3) - Consulte los límites de funcionamiento en plano","(3) - Consulte los límites de funcionamiento en plano"]
["","","","","","(4) - Consulte el diagrama de cableado y el manual de instalación para conocer el fusible correcto recomendado en función de la fuente de alimentación y la conexión a la red.","(4) - Consulte el diagrama de cableado y el manual de instalación para conocer el fusible correcto recomendado en función de la fuente de alimentación y la conexión a la red."]