{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Dimensiones","Unidad","","Altura","mm","740"]
["","","","Anchura","mm","884"]
["","","","Profundidad","mm","388"]
["Peso","Unidad","","","kg","58.5"]
["Límites de func.","Refrigeración","","Mín.","°CBS","10"]
["","","","Máx.","°CBS","43"]
["Límites de funcionamiento","Agua caliente sanitaria","","Mín.","°CBS","-25"]
["Límites de func.","Límites de func.-=-Agua caliente sanitaria","","Máx.","°CBS","35"]
["Nivel de potencia sonora","Calefacción","","Nom.","dBA","58 (1)"]
["","Refrigeración","","Nom.","dBA","61 (1)"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","44 (1)"]
["","Refrigeración","","Nom.","dBA","48 (1)"]
["Refrigerante","Tipo","","","","R-32"]
["","GWP","","","","675.0"]
["","Carga","","","tCO2Eq","1.01"]
["","Carga","","","kg","1.50"]
["Conexiones de tubería","Líquido","","D.E.","mm","6"]
["","Gas","","D.E.","mm","15.9"]
["","Drenaje","","D.E.","mm","18"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","20.0"]
["","Aislamiento térmico","","","","Tubos de líquido y de gas"]
["Alimentación eléctrica","Nombre","","","","V3"]
["","Fase","","","","1N~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","230"]
["Corriente","Fusibles recomendados","","","A","20"]
["Notas","","","","","(1) - Refrigeración Ta 35°C - LWE 18°C (DT = 5°C) - Calefacción Ta DB/WB 7°C / 6°C - LWC 35°C (DT = 5°C)"]