{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Dimensiones","Unidad","","Altura","mm","870","870"]
["","","","Anchura","mm","1,100","1,100"]
["","","","Profundidad","mm","460","460"]
["Peso","Unidad","","","kg","101","101"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","85.0","85.0"]
["","","Refrigeración","Alto","m³/min","85","85"]
["Límites de func.","Refrigeración","","Mín.","°CBS","10","10"]
["","","","Máx.","°CBS","43","43"]
["Límites de funcionamiento","Agua caliente sanitaria","","Mín.","°CBS","-25","-25"]
["Límites de func.","Límites de func.-=-Agua caliente sanitaria","","Máx.","°CBS","25 (1), 35 (1)","25 (1), 35 (1)"]
["Nivel de potencia sonora","Calefacción","","Nom.","dBA","62.0 (2)","62.0 (2)"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","48.0 (2)","48.0 (2)"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Carga","","","tCO2Eq","2.57","2.57"]
["","Carga","","","kg","3.8","3.8"]
["Conexiones de tubería","Líquido","","D.E.","mm","9.5","9.5"]
["","Gas","","D.E.","mm","15.9","15.9"]
["","Drenaje","","D.E.","mm","26","26"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","30.0","30.0"]
["","Aislamiento térmico","","","","Tubos de líquido y de gas","Tubos de líquido y de gas"]
["Alimentación eléctrica","Nombre","","","","W1","W1"]
["","Fase","","","","3~","3~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","400","400"]
["Corriente","Fusibles recomendados","","","A","16","16"]
["Notas","","","","","(1) - Encontrará más detalles en el diagrama de límites de funcionamiento.","(1) - Encontrará más detalles en el diagrama de límites de funcionamiento."]
["","","","","","(2) - Medido con una caída de presión de 10 kPa en el sistema de calefacción con unas condiciones de funcionamiento de agua de salida de 47-55°C en una habitación con una temperatura ambiente de 20°C. BS/BH 7°C/6°.","(2) - Medido con una caída de presión de 10 kPa en el sistema de calefacción con unas condiciones de funcionamiento de agua de salida de 47-55°C en una habitación con una temperatura ambiente de 20°C. BS/BH 7°C/6°."]