{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRQ-AY1"]
[]
[]
[]
[]
["","","","","","ERRQ011AAY1","ERRQ014AAY1","ERRQ016AAY1"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","52","53","55"]
["Accesorios estándar","Manual de instalación","","","","1","1","1"]
["Nivel de potencia sonora","Calefacción","","Nom.","dBA","68","69","71"]
["Refrigerante","Charge","","","TCO2Eq","9.4","9.4","9.4"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Carga","","","kg","4.5","4.5","4.5"]
["","Tipo","","","","R-410A","R-410A","R-410A"]
["Dimensiones","Unidad","","Anchura","mm","900","900","900"]
["","","","Profundidad","mm","320","320","320"]
["","","","Altura","mm","1,345","1,345","1,345"]
["Rango de funcionamiento","Calefacción","","Máx.","°CBH","20","20","20"]
["","","","Mín.","°CBH","-20","-20","-20"]
["","Agua caliente sanitaria","","Mín.","°CBS","-20","-20","-20"]
["","","","Máx.","°CBS","35","35","35"]
["Peso","Unidad","","","kg","120","120","120"]
["Conexiones de tubería","Aislamiento térmico","","","","Tubos de líquido y de gas","Tubos de líquido y de gas","Tubos de líquido y de gas"]
["","Liquid","","OD","mm","9.52","9.52","9.52"]
["","Gas","","D.E.","mm","15.9","15.9","15.9"]
["","Drain","","OD","mm","26x3","26x3","26x3"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","30","30","30"]
["Power supply","Fase","","","","3~","3~","3~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Nombre","","","","Y1","Y1","Y1"]
["","Tensión","","","V","380-415","380-415","380-415"]
["Corriente","Fusibles recomendados","","","A","16","16","16"]
["Notas","","","","","(1) - Consulte la ilustración por separado para el rango de funcionamiento","(1) - Consulte la ilustración por separado para el rango de funcionamiento","(1) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(2) - Contiene gases fluorados de efecto invernadero","(2) - Contiene gases fluorados de efecto invernadero","(2) - Contiene gases fluorados de efecto invernadero"]