{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERWQ-AV3"]
[]
[]
[]
[]
["","","","","","ERWQ02AAV3"]
["Dimensiones","Unidad","","Altura","mm","550"]
["","","","Anchura","mm","765"]
["","","","Profundidad","mm","285"]
["Peso","Unidad","","","kg","35"]
["Rango de funcionamiento","Agua caliente sanitaria","","Máx.","°CBS","35"]
["","","","Mín.","°CBS","-15"]
["Conexiones de tubería","Liquid","","OD","mm","6.35"]
["","Gas","","D.E.","mm","9.5"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","47"]
["","Refrigeración","","Nom.","dBA","47"]
["Refrigerante","Tipo","","","","R-410A"]
["","GWP","","","","2,087.5"]
["","Carga","","","kg","1.05"]
["Power supply","Nombre","","","","V3"]
["","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","230"]
["Notas","","","","","(1) - Contiene gases fluorados de efecto invernadero"]