{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH16E"]
[]
[]
[]
[]
["","","","","","ETSH16P50EF","ETSH16P30EF"]
["Carcasa","Color","","","","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)"]
["","Material","","","","Polipropileno resistente a impactos","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","","Altura","mm","1,910","1,892"]
["","","","Anchura","mm","792","594"]
["","","","Profundidad","mm","816","644"]
["Peso","Unidad","","","kg","98","75"]
["Nivel de potencia sonora","Nom.","","","dBA","45.6","45.6"]
["Nivel de presión sonora","Nom.","","","dBA","32.8","32.8"]
["Límites de funcionamiento","Calefacción","Lado del agua","Min.","°C","0 (2)","0 (2)"]
["","","","Máx.","°C","0 (2)","0 (2)"]
["","Refrigeración","Ambiente","Mín.","°CBS","0 (2)","0 (2)"]
["","","Lado del agua","Mín.","°C","0 (2)","0 (2)"]
["","","","Máx.","°C","0 (2)","0 (2)"]
["Power supply","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","230","230"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]
["","","","","","(2) - Consulte los gráficos de los límites de funcionamiento","(2) - Consulte los gráficos de los límites de funcionamiento"]