{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB-D"]
[]
[]
[]
[]
["","","","","","ETSHB16P50DA","ETSHB16P30DA"]
["Nivel de presión sonora","Nom.","","","dBA","32.8","32.8"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","10","10"]
["","","Lado del agua","Máx.","°C","22","22"]
["","","","Mín.","°C","5","5"]
["","Calefacción","Lado del agua","Máx.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Nivel de potencia sonora","Nom.","","","dBA","45.6","45.6"]
["Dimensiones","Unidad","","Anchura","mm","785","590"]
["","","","Profundidad","mm","785","615"]
["","","","Altura","mm","1,896","1,891"]
["Carcasa","Material","","","","Polipropileno resistente a impactos","Polipropileno resistente a impactos"]
["","Colour","","","","Blanco tráfico (RAL9016) / Gris oscuro (RAL7011)","Blanco tráfico (RAL9016) / Gris oscuro (RAL7011)"]
["PED","Categoría","","","","Art. 4.3","Art. 4.3"]
["Peso","Unidad","","","kg","96","75"]
["Power supply","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","230","230"]
["Calentador eléctrico","Alimentación eléctrica","","Frecuencia","Hz","50","50"]
["","","","Nombre","","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃","(4) - TKW = 10°C/TWW = 40°C/TSP = 65℃"]