{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":17,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX12E / EPRA08-12EV"]
[]
[]
[]
[]
["","","","","","ETSX12P30EF / EPRA08EAV3","ETSX12P50EF / EPRA08EAV3","ETSX12P30EG / EPRA08EAV3","ETSX12P50EG / EPRA08EAV3","ETSX12P30EF / EPRA10EAV3","ETSX12P50EF / EPRA10EAV3","ETSX12P50EG / EPRA10EAV3","ETSX12P30EG / EPRA10EAV3","ETSX12P30EF / EPRA12EAV3","ETSX12P50EF / EPRA12EAV3","ETSX12P30EG / EPRA12EAV3","ETSX12P50EG / EPRA12EAV3"]
["Indoor unit","","","","","ETSX12P30EF","ETSX12P50EF","ETSX12P30EG","ETSX12P50EG","ETSX12P30EF","ETSX12P50EF","ETSX12P50EG","ETSX12P30EG","ETSX12P30EF","ETSX12P50EF","ETSX12P30EG","ETSX12P50EG"]
["Capacidad de calefacción","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Capacidad de refrigeración","Nom.","","","kW","6.81 (2)","6.81 (2)","6.81 (2)","6.81 (2)","7.97 (2)","7.97 (2)","7.97 (2)","7.97 (2)","8.62 (2)","8.62 (2)","8.62 (2)","8.62 (2)"]
["Consumo","Calefacción","","Nom.","kW","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)"]
["","Refrigeración","","Nom.","kW","2.15 (2)","2.15 (2)","2.15 (2)","2.15 (2)","2.66 (2)","2.66 (2)","2.66 (2)","2.66 (2)","2.96 (2)","2.96 (2)","2.96 (2)","2.96 (2)"]
["COP","","","","","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)"]
["EER","","","","","3.17 (2)","3.17 (2)","3.17 (2)","3.17 (2)","3","3","3.00 (2)","3.00 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)"]
["Calentamiento de agua caliente sanitaria","General","","Perfil de carga declarado","","L","XL","L","XL","L","XL","XL","L","L","XL","L","XL"]
["","Clima medio","","Clase de eficiencia energética de calentamiento de agua","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 55°C","General","SCOP","","3.47","3.47","3.47","3.47","3.48","3.48","3.48","3.48","3.48","3.48","3.48","3.48"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","Clase de efic. estac. de calef. de habitaciones","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 35°C","General","SCOP","","4.79","4.79","4.79","4.79","4.82","4.82","4.82","4.82","4.82","4.82","4.82","4.82"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 35°C","General","Clase de efic. estac. de calef. de habitaciones","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Rango de eficiencia energética","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notas","","","","","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condición 1: refrigeración Ta 35°C - LWE 18°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Condición 2: refrigeración Ta 35°C - LWE 7°C (DT = 5°C); calefacción Ta BS/BH 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condición: Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad","(4) - BS/BH 7°C/6°C - LWC 35°C (dT=5°C) con bomba a máxima velocidad"]