{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWHT-Q-XSA"]
[]
[]
[]
[]
["","","","","","EWHT100Q-XSA1"]
["Capacidad de refrigeración","Nom.","","","kW","91.68"]
["Control de capacidad","Método","","","","Etapa"]
["","Capacidad mínima","","","%","50"]
["Consumo","Refrigeración","","Nom.","kW","21.22"]
["EER","","","","","4.32"]
["IPLV","","","","","6.66"]
["SEER","","","","","5.98"]
["Dimensiones","Unidad","","Profundidad","mm","1300"]
["","","","Altura","mm","1000"]
["","","","Anchura","mm","1200"]
["Peso","Peso operativo","","","kg","451"]
["","Unidad","","","kg","431"]
["Carcasa","Color","","","","Blanco marfil"]
["","Material","","","","Acero galvanizado"]
["Intercambiador de calor de agua: evaporador","Caída de presión del agua","Refrigeración","Nom.","kPa","17.7"]
["Compresor","Cantidad","","","","2"]
["","Tipo","","","","Scroll"]
["Límites de funcionamiento","Lado del agua","Evaporador","Mín.","°CBS","-15"]
["","","","Máx.","°CBS","30"]
["Nivel de potencia sonora","Refrigeración","","Nom.","dBA","80.99"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","65.4"]
["Refrigerante","Tipo","","","","R-32"]
["","GWP","","","","675"]
["","Carga","","","kg","7"]
["","Circuitos","","Cantidad","","1"]
["Conexiones de tubería","Entrada/salida de agua del evaporador (D.E.)","","","","3\""]
["Alimentación eléctrica","Fase","","","","3"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","400"]
["","Límites de tensión","","Mín.","%","-10"]
["","","","Máx.","%","+10"]
["Unidad","Corriente de arranque","","Máx.","A","221"]
["","Corriente de func.","Refrigeración","Nom.","A","36.9"]
["","","","Máx.","A","62"]
["","Corriente de la unidad máx. para el tamaño de los cables","","","A","68"]