{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A / ARXM-N9"]
[]
[]
[]
[]
["","","","","FAA71AUVEB / ARXM71N2V1B9"]
["Capacidad de refrigeración","Nom.","","kW","6.80"]
["","Máx.","","kW","6.95"]
["Capacidad de calefacción","Nom.","","kW","7.50"]
["","Máx.","","kW","7.59"]
["Eficiencia nominal","EER","","","3.40"]
["","COP","","","3.19"]
["","Consumo energético anual","","kWh","1000"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A"]
["","","Calefacción","","D"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A+"]
["","Capacidad","Pdesign","kW","6.80"]
["","SEER","","","5.77"]
["","Consumo energético anual","","kWh/a","412"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A"]
["","Capacidad","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Capacidad de calefacción Pdh a -10°","","kW","4.50"]
["","Consumo energético anual","","kWh/a","1652"]
["Rango de eficiencia energética","","","","A+++ ~ D"]
["Notas","","","","(1) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(2) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","(3) - Capacidades nom. de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","(4) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]