{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FAA100AUVEB / AZAS100M7V1B","FAA71AUVEB / AZAS71M2V1B (Archived)"]
["Capacidad de refrigeración","Nom.","","kW","9.50 (1)","6.80 (1)"]
["Refrigeración de habitaciones","SEER","","","5.25","5.77"]
["","Consumo energético anual","","kWh/a","633","412"]
["","Capacidad","Pdesign","kW","9.50","6.80"]
["","Clase de eficiencia energética","","","A","A+"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","6.00","4.50"]
["","SCOP/A","","","3.81","3.81"]
["","Clase de eficiencia energética","","","A","A"]
["","Consumo energético anual","","kWh/a","2,205","1,654"]
["Capacidad de calefacción","Nom.","","kW","10.8 (2)","7.50 (2)"]
["Notas","","","","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m.","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m.","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(4) - Consulte en el plano independiente con los datos eléctricos.","(4) - Consulte en el plano independiente con los datos eléctricos."]