{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9 / RZQSG71L3V1B","FAQ100CVEB9 / RZQSG100L9V1B"]
["Capacidad de refrigeración","Nom.","","kW","6.8","9.5"]
["Refrigeración de habitaciones","SEER","","","5.81","5.61"]
["","Consumo energético anual","","kWh/a","410","593"]
["","Capacidad","Pdesign","kW","6.8","9.50"]
["","Clase de eficiencia energética","","","A+","A+"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","6.33","6.81"]
["","SCOP/A","","","3.90","4.01"]
["","Clase de eficiencia energética","","","A","A+"]
["","Consumo energético anual","","kWh/a","2,273","2,378"]
["Eficiencia nominal","Consumo energético anual","","kWh","1,059","1,580"]
["","EER","","","3.21","3.01"]
["","COP","","","3.61","3.41"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","B"]
["","","Calefacción","","A","B"]
["Capacidad de calefacción","Nom.","","kW","7.5","10.8"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]