{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 3MXM-A"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 3MXM68A2V1B"]
["Capacidad de refrigeración","Nom.","","kW","6.80"]
["Eficiencia nominal","Annual energy consumption","","kWh","1,245"]
["","EER","","","2.73"]
["","COP","","","3.24"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","D"]
["","","Calefacción","","C"]
["Capacidad de calefacción","Nom.","","kW","8.60"]
["Notas","","","","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(4) - Consulte en el plano independiente con los datos eléctricos."]