{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 4MXM-A9"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 4MXM68A2V1B9"]
["Capacidad de refrigeración","Nom.","","kW","6.8"]
["Capacidad de calefacción","Nom.","","kW","8.60"]
["Eficiencia nominal","EER","","","2.73"]
["","COP","","","3.24"]
["","Consumo energético anual","","kWh","1245"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","D"]
["","","Calefacción","","C"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A"]
["","Capacidad","Pdesign","kW","6.80"]
["","SEER","","","5.26"]
["","Consumo energético anual","","kWh/a","453"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A"]
["","Capacidad","Pdesign","kW","3.60"]
["","SCOP/A","","","3.81"]
["","Capacidad de calefacción Pdh a -10°","","kW","3.10"]
["","Consumo energético anual","","kWh/a","1323"]