{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXM50A5V1B","FBA60A2VEB9 / RXM60A5V1B"]
["Capacidad de refrigeración","Nom.","","kW","5.0","5.7"]
["Capacidad de calefacción","Nom.","","kW","5.5","7"]
["Eficiencia nominal","EER","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Consumo energético anual","","kWh","704","819"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A"]
["","","Calefacción","","A","A"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A++","A+"]
["","Capacidad","Pdesign","kW","5.0","5.7"]
["","SEER","","","6.27","5.91"]
["","Consumo energético anual","","kWh/a","279","336"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A+","A+"]
["","Capacidad","Pdesign","kW","4.4","4.6"]
["","SCOP/A","","","4.06","4.01"]
["","Capacidad de calefacción Pdh a -10°","","kW","3.73","3.99"]
["","Consumo energético anual","","kWh/a","1,517","1607"]
["Notas","","","","","(1) - Capacidades nom. de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(4) - Consulte en el plano independiente con los datos eléctricos."]