{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Unidad exterior","","","","AZAS71M2V1B"]
["Capacidad de refrigeración","Nom.","","kW","6.80"]
["Capacidad de calefacción","Nom.","","kW","7.50"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A"]
["","Capacidad","Pdesign","kW","6.80"]
["","SEER","","","5.57"]
["","Consumo energético anual","","kWh/a","427"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A"]
["","Capacidad","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Consumo energético anual","","kWh/a","1654"]
["Notas","","","","(1) - Refrigeración: T2: temp. interior 26,6°CBS, 19,4°CBH; temp. exterior 48 °CBS [Btu/h/W]"]
["","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]