{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ71C8VEB / RZQSG71L3V1B","FBQ100C8VEB / RZQSG100L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L9V1B","FBQ125C8VEB / RZQSG125L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L9V1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L9V1B"]
["Capacidad de refrigeración","Nom.","","kW","6.8","9.5","","","","12.0"]
["Refrigeración de habitaciones","SEER","","","5.81","5.50","5.10","5.10","4.80","5.20","4.80","4.80"]
["","Consumo energético anual","","kWh/a","410","605","652","652","875","808","875","875"]
["","Capacidad","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Clase de eficiencia energética","","","A+","A","B","B","B","A","B","B"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.88","4.01","3.80","3.80","3.80","3.90","3.80","3.80"]
["","Clase de eficiencia energética","","","A","A+","A","A","A","A","A","A"]
["","Consumo energético anual","","kWh/a","2,166","2,654","2,800","2,800","2,800","2,729","2,800","2,800"]
["Eficiencia nominal","Consumo energético anual","","kWh","1,035","1,435","","","","1,870"]
["","EER","","","3.28","3.31","","","","3.21"]
["","COP","","","3.61","3.65","","","","3.51"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A","","","","A"]
["","","Calefacción","","A","A","","","","B"]
["Capacidad de calefacción","Nom.","","kW","7.5","10.8","","","","13.5"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]
["","","","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]