{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ50D2VEB / RXS50L2V1B","FBQ60D2VEB / RXS60L2V1B (Archived)"]
["Capacidad de refrigeración","Nom.","","kW","5.0 (2)"]
["Eficiencia nominal","Consumo energético anual","","kWh","710"]
["","EER","","","3.52 (1)"]
["","COP","","","3.83 (1)"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A"]
["","","Calefacción","","A"]
["Capacidad de calefacción","Nom.","","kW","5.50 (2)"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]
["Outdoor unit","","","","","RXS60L"]
["Capacidad de refrigeración","Nom.","","kW","","5.7"]
["Capacidad de calefacción","Nom.","","kW","","7.00"]
["Eficiencia nominal","EER","","","","3.45"]
["","COP","","","","3.71"]
["","Consumo energético anual","","kWh","","826"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","A"]
["","","Calefacción","","","A"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","","A+"]
["","Capacidad","Pdesign","kW","","5.70"]
["","SEER","","","","5.86"]
["","Consumo energético anual","","kWh/a","","340"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","","A+"]
["","Capacidad","Pdesign","kW","","4.60"]
["","SCOP/A","","","","4.01"]
["","Consumo energético anual","","kWh/a","","1606"]