{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B","FCAG140AVEB / RZQG140L7Y1B"]
["Capacidad de refrigeración","Nom.","","kW","","","","","","","","","","","","","6.80 (1)","","","13.4 (1)","13.4 (1)"]
["Refrigeración de habitaciones","SEER","","","","","","","","","","","","","5.10","5.10","6.72","","","9.70","6.44"]
["","ηs,c","","%","","","","","","","","","","","","","","","","385.1","254.6"]
["","Consumo energético anual","","kWh/a","","","","","","","","","","","467","467","355","","","829","1,249"]
["","Capacidad","Pdesign","kW","","","","","","","","","","","6.80","6.80","6.80","","","13.4","13.4"]
["","Clase de eficiencia energética","","","","","","","","","","","","","A","A","A++"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","","","","","","","","","","","6.00","6.00","6.33","","","12.0","11.6"]
["","SCOP/A","","","","","","","","","","","","","3.80","3.80","4.20","","","3.96","4.27"]
["","Clase de eficiencia energética","","","","","","","","","","","","","A","A","A+"]
["","Consumo energético anual","","kWh/a","","","","","","","","","","","2,211","2,211","2,110","","","4,235","3,795"]
["","ηs,h","","%","","","","","","","","","","","","","","","","155.2","167.6"]
["Eficiencia nominal","Annual energy consumption","","kWh","","","","","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","","","","","3.39 (3)","","","4.29 (3)","2.50 (3)"]
["","COP","","","","","","","","","","","","","","","3.97 (3)","","","","3.61 (3)"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","","","","","","","","","","","A"]
["","","Calefacción","","","","","","","","","","","","","","A"]
["Capacidad de calefacción","Nom.","","kW","","","","","","","","","","","","","7.50 (2)","","","15.5 (2)","15.5 (2)"]
["Notas","","","","","","","","","","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","","","","","","","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","","","","","","","","","","","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["Rango de eficiencia energética","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D"]
["Outdoor unit","","","","","","","","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","","","","","","","","","","","","","","A","A"]
["","Capacidad","Pdesign","kW","","","","","","","","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10"]
["","Consumo energético anual","","kWh/a","","","","","","","","","","","","","","652","824"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","","","","","","","","","","","","","","A","A"]
["","Capacidad","Pdesign","kW","","","","","","","","","","","","","","11.3","12.7"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80"]
["","Consumo energético anual","","kWh/a","","","","","","","","","","","","","","4164","4683"]