{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXS35L3V1B"]
["Capacidad de refrigeración","Nom.","","kW","3.40"]
["Capacidad de calefacción","Nom.","","kW","4.20"]
["Eficiencia nominal","Consumo energético anual","","kWh","455"]
["","COP","","","3.50"]
["","EER","","","3.74"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A"]
["","","Calefacción","","B"]
["Conexiones de tubería","Drenaje","D.E.","mm","VP25 (Diá. ext. 32, diá. int. 25)"]
["","Gas","D.E.","mm","9.50"]
["","Líquido","D.E.","mm","6.35"]
["Notas","","","","(1) - Durante el funcionamiento normal: +22°C / + 32°C"]
["","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(4) - Consulte en el plano independiente con los datos eléctricos."]