{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":13,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Capacidad de refrigeración","Nom.","","kW","","","","","","","","6.80 (1)","13.4 (1)"]
["Refrigeración de habitaciones","SEER","","","","","","","","","6.91","6.91","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Consumo energético anual","","kWh/a","","","","","","","345","345","1,191"]
["","Capacidad","Pdesign","kW","","","","","","","6.80","6.80","13.4"]
["","Clase de eficiencia energética","","","","","","","","","A++","A++"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","","","","","","","7.60","7.60","11.8"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Clase de eficiencia energética","","","","","","","","","A+","A+"]
["","Consumo energético anual","","kWh/a","","","","","","","2,344","2,344","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Eficiencia nominal","Consumo energético anual","","kWh","","","","","","","","830"]
["","EER","","","","","","","","","","4.09 (3)","3.18 (3)"]
["","COP","","","","","","","","","","4.80 (3)","4.12 (3)"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","","","","","","A"]
["","","Calefacción","","","","","","","","","A"]
["Capacidad de calefacción","Nom.","","kW","","","","","","","","7.50 (2)","15.5 (2)"]
["Rango de eficiencia energética","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notas","","","","","","","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","","","","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","","","","","","","","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]