{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQG71L8Y1B","FCQG100FVEB / RZQG71L8Y1B","FCQG71FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG140L7Y1B"]
["Capacidad de refrigeración","Nom.","","kW","","","6.8","","","","","","","13.4"]
["Refrigeración de habitaciones","SEER","","","5.1","6.80","6.72","5.10","6.80","5.10","5.10","5.10","6.00"]
["","Consumo energético anual","","kWh/a","467","350","355","652","489","652","652","824","700"]
["","Capacidad","Pdesign","kW","6.8","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Clase de eficiencia energética","","","B","A++","A++","B","A++","B","B","B","A+"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","6","6.33","6.33","11.30","11.30","11.30","11.30","12.71","12.66"]
["","SCOP/A","","","3.8","4.20","4.20","3.80","4.61","3.80","3.80","3.80","4.10"]
["","Clase de eficiencia energética","","","A","A+","A+","A","A++","A","A","A","A+"]
["","Consumo energético anual","","kWh/a","2,211","2,110","2,110","4,164","3,432","4,164","4,164","4,683","4,323"]
["Eficiencia nominal","Consumo energético anual","","kWh","","","1,005"]
["","EER","","","","","3.39","","","","","","","3.21"]
["","COP","","","","","3.97","","","","","","","3.61"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","A"]
["","","Calefacción","","","","A"]
["Capacidad de calefacción","Nom.","","kW","","","7.5","","","","","","","15.5"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","","","(1) - Consumo anual de energía de acuerdo con la Directiva de etiquetado energético 2002/31/EC","","","","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","","","(2) - SEER y SCOP conforme a EN 14825","","","","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]