{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","12.10","19.00","22.00"]
["Capacidad de calefacción","Capacidad total","","Nom.","kW","13.50","22.4","24.0"]
["Carcasa","Color","","","","Sin pintar","Sin pintar","Sin pintar"]
["","Material","","","","Acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado"]
["Dimensiones","Unidad","","Altura","mm","300","470","470"]
["","","","Anchura","mm","1,400","1,490","1,490"]
["","","","Profundidad","mm","700","1,100","1,100"]
["Peso","Unidad","","","kg","45","104","115"]
["Espacio necesario en el falso techo >","mm","","","","350"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","39.0","64.0","69.0"]
["","","","Medio","m³/min","","50","56"]
["","","","Bajo","m³/min","28.0","36.0","43.0"]
["","","Calefacción","Alto","m³/min","39.0","64.0","69.0"]
["","","","Medio","m³/min","","50.0","56.0"]
["","","","Bajo","m³/min","28.0","36.0","43.0"]
["","Presión estática externa","","Alto","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Nivel de potencia sonora","Refrigeración","","","dBA","66","69.0","71.0"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","40","43.0","44.0"]
["","","","Medio","dBA","","39.0","40.0"]
["","","","Bajo","dBA","33","36.0","37.0"]
["","Calefacción","","Alto","dBA","40","43.0","44.0"]
["","","","Medio","dBA","","39.0","40.0"]
["","","","Bajo","dBA","33","36.0","37.0"]
["Conexiones de tubería","Líquido","","D.E.","mm","9.52","9.52","9.52"]
["","Gas","","D.E.","mm","15.90","19.1","22.2"]
["","Drenaje","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Altura de drenaje","mm","","","","625"]
["Panel decorativo","Modelo","","","","BYBS125DJW1"]
["","Color","","","","Blanco (10Y9/0,5)"]
["","Dimensiones","","Altura","mm","55"]
["","","","Anchura","mm","1,500"]
["","","","Profundidad","mm","500"]
["","Peso","","","kg","6.5"]
["Sistemas de control","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accesorios estándar","Manual de uso","","","","","1","1"]
["","Manual de instalación y de uso","","","","1","1","1"]
["","Manual de instalación","","","","","1","1"]
["","Precauciones generales de seguridad","","","","1","1","1"]
["","Tubo de conexión del gas","","","","","1","1"]
["","Material de la abrazadera para cables","","","","","1","1"]
["","Arandela","","","","8","12","12"]
["","Arandela elástica","","","","","2","2"]
["","Tornillo+Arandela","","","","","45","45"]
["","Tornillo hexagonal con arandela","","","","","49","49"]
["","Tornillos","","","","16","2","2"]
["","Tornillo hexagonal","","","","","2","2"]
["","Arandela plana","","","","","8","8"]
["Power supply","Nombre","","","","","VE","VE"]
["","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50/60","50/60","50/60"]
["","Tensión","","","V","220-240/220","220-240/220","220-240/220"]
["Accesorios estándar","Abrazadera de tubo flexible","","","","1"]
["","Tubo flexible de drenaje","","","","1"]
["","Cable para alimentación eléctrica común","","","","2"]
["","Material de sellado (manguera de drenaje)","","","","1"]
["","Material de sellado","","","","2"]
["","Tubo de aislamiento térmico (líquido)","","","","1"]
["","Tubo de aislamiento térmico (gas)","","","","1"]
["Notas","","","","","(1) - Consulte en el plano independiente con los datos eléctricos."]