{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","35.0","35.0"]
["","","","Bajo","dBA","29.0","29.0"]
["","Refrigeración","","Bajo","dBA","28.0","28.0"]
["","","","Alto","dBA","35.0","35.0"]
["Accesorios estándar","Manual de instalación y de uso","","","","1","1"]
["","Filtro de aire de aspiración","","","","1","1"]
["Sistemas de control","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","D.E.","mm","9.52"]
["","Drain","","","","27.2"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55","55"]
["","Calefacción","","","dBA","55","55"]
["Dimensiones","Unidad","","Anchura","mm","652","652"]
["","","","Profundidad","mm","502","502"]
["","","","Altura","mm","230","230"]
["Carcasa","Material","","","","Acero bajo en carbono cincado","Acero bajo en carbono cincado"]
["Peso","Unidad","","","kg","17.0","17.0"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","6.95"]
["","","","Bajo","m³/min","","5.20"]
["","","Refrigeración","Bajo","m³/min","","5.20"]
["","","","Alto","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Nombre","","","","V1","V1"]
["","Tensión","","","V","230","230 +/-10%"]
["Notas","","","","","(1) - Los valores de sonido se calculan en una cámara semianecoica.","(1) - Los valores de sonido se calculan en una cámara semianecoica."]
["","","","","","(2) - El nivel de presión sonora es un valor relativo que depende de la distancia y del entorno acústico. Para más detalles, consulte los esquemas de nivel sonoro.","(2) - El nivel de presión sonora es un valor relativo que depende de la distancia y del entorno acústico. Para más detalles, consulte los esquemas de nivel sonoro."]
["","","","","","(3) - El nivel de potencia sonora es un valor absoluto que indica la potencia que genera una fuente de sonido.","(3) - El nivel de potencia sonora es un valor absoluto que indica la potencia que genera una fuente de sonido."]
["Piping connections","Liquid","","OD","mm","","6.35"]
["","Gas","","D.E.","mm","","9.52"]
["","Drain","","","","","27.2"]