{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB","FDQ125C7VEB"]
["Nivel de presión sonora","Calefacción","Alto","dBA","40","40"]
["","","Bajo","dBA","33","33"]
["","Refrigeración","Bajo","dBA","33","33"]
["","","Alto","dBA","40","40"]
["Sistemas de control","Controlador remoto con cable","","","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D528"]
["","Infrared remote control","","","BRC4C65","BRC4C65"]
["Capacidad de refrigeración","Capacidad total","Nom.","kW","12.5 (1)","12.5"]
["Conexiones de tubería","Liquid","OD","mm","9.52","9.52"]
["","Gas","D.E.","mm","15.9","15.9"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Power input","Refrigeración","Nom.","kW","0.35"]
["","Calefacción","Nom.","kW","0.35"]
["Espacio necesario en el falso techo >","mm","","","350","350"]
["Sound power level","Refrigeración","","dBA","66","66"]
["Dimensiones","Unidad","Anchura","mm","1,400","1,400"]
["","","Profundidad","mm","700","700"]
["","","Altura","mm","300","300"]
["Carcasa","Material","","","","Acero galvanizado"]
["","Color","","","No pintada (galvanizada)","Not painted"]
["Peso","Unidad","","kg","45","45"]
["Ventilador","Presión estática externa","Alto","Pa","200","200"]
["","","Nom.","Pa","50","50"]
["Altura de drenaje","mm","","","625","625"]
["Panel decorativo","Peso","","kg","6.5","6.5"]
["","Modelo","","","BYBS125DJW1","BYBS125DJW1"]
["","Dimensiones","Altura","mm","55","55"]
["","","Profundidad","mm","500","500"]
["","","Anchura","mm","1,500","1,500"]
["","Color","","","Blanco (10Y9/0,5)","Blanco (10Y9/0,5)"]
["Capacidad de calefacción","Capacidad total","Nom.","kW","14.0 (2)","14.0"]
["Power supply","Fase","","","1~","1~"]
["","Frecuencia","","Hz","50/60","50/60"]
["","Nombre","","","VE","VE"]
["","Tensión","","V","220-240/220","220-240/220"]
["Notas","","","","(1) - Refrigeración: temp. interior 27°CBS / 19,0°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5m; diferencia de nivel: 0m","(1) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m","(2) - Las capacidades son netas, incluida una deducción para la refrigeración (y una adición para la calefacción) debido al calor del motor del ventilador."]
["","","","","(3) - Las capacidades son netas, incluida una deducción para la refrigeración (y una adición para la calefacción) debido al calor del motor del ventilador.","(3) - Los valores de presión sonora corresponden a una unidad instalada con aspiración posterior."]
["","","","","(4) - Los valores de presión sonora corresponden a una unidad instalada con aspiración posterior.","(4) - Categoría de unidad PED: excluida del ámbito de aplicación PED debido al artículo 1, elemento 3.6 de 97/23/EC"]
["","","","","(5) - Categoría de unidad PED: excluida del ámbito de aplicación PED debido al artículo 1, elemento 3.6 de 97/23/EC","(5) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5m (horizontal); diferencia de nivel 0m"]