{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXM50A5V1B","FDXM60F3V1B9 / RXM60A5V1B"]
["Capacidad de refrigeración","Mín.","","kW","1.70","1.7"]
["","Nom.","","kW","5.00","6"]
["","Máx.","","kW","5.30","6.5"]
["Capacidad de calefacción","Mín.","","kW","1.70","1.7"]
["","Nom.","","kW","5.80","7"]
["","Máx.","","kW","6.00","7.1"]
["Eficiencia nominal","EER","","","3.06","2.93"]
["","COP","","","3.10","3.21"]
["","Consumo energético anual","","kWh","817","1024"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","B","C"]
["","","Calefacción","","D","C"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","A+","A"]
["","Capacidad","Pdesign","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Consumo energético anual","","kWh/a","303","378"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","A","A"]
["","Capacidad","Pdesign","kW","4.00","4.6"]
["","SCOP/A","","","3.93","3.8"]
["","Capacidad de calefacción Pdh a -10°","","kW","3.54","3.94"]
["","Consumo energético anual","","kWh/a","1424","1693"]
["Notas","","","","","(1) - Capacidades nom. de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(4) - Consulte en el plano independiente con los datos eléctricos."]