{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / RXS50L2V1B"]
["Capacidad de refrigeración","Mín.","","kW","1.7"]
["","Máx.","","kW","5.3"]
["","Nom.","","kW","5.0"]
["Conexiones de tubería","Liquid","OD","mm","6.35"]
["","Gas","D.E.","mm","12.7"]
["","Drain","OD","mm","VP20 (Diá. ext. 26, diá. int. 20)"]
["Eficiencia nominal","Annual energy consumption","","kWh","825"]
["","EER","","","3.03"]
["","COP","","","3.10"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","B"]
["","","Calefacción","","D"]
["Capacidad de calefacción","Nom.","","kW","5.8"]
["","Mín.","","kW","1.7"]
["","Máx.","","kW","6.0"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(2) - 230V"]
["","","","","(3) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]