{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXS25L3V1B","FFA35A2VEB / RXS35L3V1B"]
["Capacidad de refrigeración","Nom.","","kW","2.50","3.40"]
["Refrigeración de habitaciones","SEER","","","6.11","6.32"]
["","Consumo energético anual","","kWh/a","143","188"]
["","Capacidad","Pdesign","kW","2.50","3.40"]
["","Clase de eficiencia energética","","","A++","A++"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Clase de eficiencia energética","","","A+","A+"]
["","Consumo energético anual","","kWh/a","763","1,059"]
["Conexiones de tubería","Líquido","D.E.","mm","6.35","6.35"]
["","Gas","D.E.","mm","9.50","9.50"]
["","Drain","OD","mm","VP20 (Diá. ext. 26, diá. int. 20)","VP20 (Diá. ext. 26, diá. int. 20)"]
["Eficiencia nominal","EER","","","4.53","3.78"]
["","Consumo energético anual","","kWh","276","450"]
["","COP","","","3.90","3.50"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A"]
["","","Calefacción","","A","A"]
["Capacidad de calefacción","Nom.","","kW","3.20","4.20"]
["Notas","","","","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m.","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m.","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(4) - Consulte en el plano independiente con los datos eléctricos.","(4) - Consulte en el plano independiente con los datos eléctricos."]