{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Carcasa","Material","","","","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado","Placa de acero galvanizado"]
["Dimensiones","Unidad","","Altura","mm","260","260","260","260"]
["","","","Anchura","mm","575","575","575","575"]
["","","","Profundidad","mm","575","575","575","575"]
["Peso","Unidad","","","kg","16.0","16.0","17.5","17.5"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","9.0","10.0","12.0","14.5"]
["","","","Medio","m³/min","8.0","8.5","10.0","12.5"]
["","","","Bajo","m³/min","6.5","6.5","7.5","9.5"]
["","","Calefacción","Alto","m³/min","9.0","10.0","12.0","14.5"]
["","","","Medio","m³/min","8.0","8.5","10.0","12.5"]
["","","","Bajo","m³/min","6.5","6.5","7.5","9.5"]
["Nivel de potencia sonora","Refrigeración","","","dBA","48","51","56","60"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","31.0","34.0","39.0","43.0"]
["","","","Medio","dBA","28.5","30.5","34.0","40.0"]
["","","","Bajo","dBA","25.0","25.0","27.0","32.0"]
["","Calefacción","","Alto","dBA","31.0","34.0","39.0","43.0"]
["","","","Medio","dBA","28.5","30.5","34.0","40.0"]
["","","","Bajo","dBA","25.0","25.0","27.0","32.0"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.52","9.52","12.70","12.70"]
["","Drenaje","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Panel decorativo","Modelo","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Color","","","","Blanco (N9.5)","Blanco (N9.5)","Blanco (N9.5)","Blanco (N9.5)"]
["","Dimensiones","","Altura","mm","46","46","46","46"]
["","","","Anchura","mm","620","620","620","620"]
["","","","Profundidad","mm","620","620","620","620"]
["","Peso","","","kg","2.8","2.8","2.8","2.8"]
["Panel decorativo 2","Modelo","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Color","","","","Plateado","Plateado","Plateado","Plateado"]
["","Dimensiones","","Altura","mm","46","46","46","46"]
["","","","Anchura","mm","620","620","620","620"]
["","","","Profundidad","mm","620","620","620","620"]
["","Peso","","","kg","2.8","2.8","2.8","2.8"]
["Panel decorativo 3","Modelo","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Color","","","","Blanco (RAL9010)","Blanco (RAL9010)","Blanco (RAL9010)","Blanco (RAL9010)"]
["","Dimensiones","","Altura","mm","55","55","55","55"]
["","","","Anchura","mm","700","700","700","700"]
["","","","Profundidad","mm","700","700","700","700"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Panel decorativo 4","Modelo","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Color","","","","Blanco (RAL9010)","Blanco (RAL9010)","Blanco (RAL9010)","Blanco (RAL9010)"]
["","Dimensiones","","Altura","mm","55","55","55","55"]
["","","","Anchura","mm","700","700","700","700"]
["","","","Profundidad","mm","700","700","700","700"]
["","Peso","","","kg","2.7","2.7","2.7","2.7"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)","BRC7EB530 (panel estándar), BRC7F530W (panel blanco), BRC7F530S (panel gris)"]
["","Controlador remoto con cable","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Accesorios estándar","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240"]