{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9)"]
[]
[]
[]
[]
["","","","","","FHA35AVEB99 (Archived)"]
["Carcasa","Color","","","","Blanco"]
["","Material","","","","Resina, metal laminado"]
["Dimensiones","Unidad","","Altura","mm","235"]
["","","","Anchura","mm","960"]
["","","","Profundidad","mm","690"]
["Peso","Unidad","","","kg","24.0"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","14.0"]
["","","","Medio","m³/min","11.5"]
["","","","Bajo","m³/min","10.0"]
["","","Calefacción","Alto","m³/min","14.0"]
["","","","Medio","m³/min","11.5"]
["","","","Bajo","m³/min","10.0"]
["Nivel de potencia sonora","Refrigeración","","","dBA","53"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","36"]
["","","","Medio","dBA","34"]
["","","","Bajo","dBA","31"]
["","Calefacción","","Alto","dBA","36"]
["","","","Medio","dBA","31"]
["","","","Nom.","dBA","34"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.40"]
["","Gas","","D.E.","mm","9.50"]
["","Drenaje","","","","VP20"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","BRC7GA53, BRC7GA56"]
["","Controlador remoto con cable","","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["Accesorios estándar","Thermal insulation tube","","","","2"]
["","Resin bushing","","","","1"]
["","Wiring fixture","","","","2"]
["","Hose band","","","","1"]
["","Wire clamp material","","","","7"]
["","Drain hose","","","","1"]
["","Screws","","","","2"]
["","Sealing pad (large)","","","","1"]
["","Sealing pad (small)","","","","1"]
["","Washer","","","","8"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]
["Notas","","","","","(1) - Consulte en el plano independiente con los datos eléctricos."]