{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":23,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9)"]
[]
[]
[]
[]
["","","","","","FHA50AVEB9","FHA50AVEB98","FHA60AVEB9","FHA60AVEB99","FHA60AVEB98","FHA71AVEB9","FHA71AVEB98","FHA100AVEB9","FHA100AVEB8","FHA100AVEB","FHA125AVEB","FHA125AVEB8","FHA125AVEB9","FHA140AVEB","FHA140AVEB8","FHA140AVEB9","FHA35AVEB99 (Archived)","FHA35AVEB98 (Archived)"]
["Capacidad de refrigeración","Capacidad total","","Nom.","kW","","","","","","","","","","","","14.00","","","15.40"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco","","Blanco","","Blanco","Blanco","Blanco","Blanco","","Blanco","","","Blanco","","Blanco","Blanco"]
["","Material","","","","Resina, metal laminado","Resina, metal laminado","Resina, metal laminado","","Resina, metal laminado","","Resina, metal laminado","Resina, metal laminado","Resina, metal laminado","Resina, metal laminado","","Resina, metal laminado","","","Resina, metal laminado","","Resina, metal laminado","Resina, metal laminado"]
["Dimensiones","Unidad","","Altura","mm","235","235","235","","235","","235","235","235","235","","235","","","235","","235","235"]
["","","","Anchura","mm","960","960","1270","","1270","","1270","1590","1590","1590","","1590","","","1590","","960","960"]
["","","","Profundidad","mm","690","690","690","","690","","690","690","690","690","","690","","","690","","690","690"]
["Peso","Unidad","","","kg","25","27","31","31.0","32","32","34","38.0","41","38.0","38.0","41","38.0","38.0","41","38.0","24.0","26"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","15.0","15.0","19.5","","19.5","","20.5","28.0","28.0","28.0","","31.0","","","34.0","","14.0","14.0"]
["","","","Medio","m³/min","12.0","12.0","15.0","","15.0","","17.0","24.0","24.0","24.0","","27.0","","","29.0","","11.5","11.5"]
["","","","Bajo","m³/min","10.0","10.0","11.5","","11.5","","14.0","20.0","20.0","20.0","","23.0","","","24.0","","10.0","10.0"]
["","","Calefacción","Alto","m³/min","15.0","15.0","19.5","","19.5","","20.5","28.0","28.0","28.0","","31.0","","","34.0","","14.0","14.0"]
["","","","Medio","m³/min","12.0","12.0","15.0","","15.0","","17.0","24.0","24.0","24.0","","27.0","","","29.0","","11.5","11.5"]
["","","","Bajo","m³/min","10.0","10.0","11.5","","11.5","","14.0","20.0","20.0","20.0","","23.0","","","24.0","","10.0","10.0"]
["Nivel de potencia sonora","Refrigeración","","","dBA","54.0","54.0","54.0","","54.0","","55.0","60","60.0","60","","62.0","","","64.0","","53","53.0"]
["","Calefacción","","","dBA","","54.0","","","54.0","","55.0","","60.0","","","62.0","","","64.0","","","53.0"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","37.0","37.0","37.0","","37.0","","38.0","42","42.0","42","","44.0","","","46.0","","36","36.0"]
["","","","Medio","dBA","35.0","35.0","35.0","","35.0","","36.0","38","38.0","38","","41.0","","","42.0","","34","34.0"]
["","","","Bajo","dBA","32.0","32.0","33.0","","33.0","","34.0","34","34.0","34","","37.0","","","38.0","","31","31.0"]
["","Calefacción","","Alto","dBA","37.0","37.0","37.0","","37.0","","38.0","42","42.0","42","","44.0","","","46.0","","36","36.0"]
["","","","Medio","dBA","32.0","32.0","33.0","","33.0","","34.0","34","34.0","34","","37.0","","","38.0","","31","31.0"]
["","","","Nom.","dBA","35.0","35.0","35.0","","35.0","","36.0","38","38.0","38","","41.0","","","42.0","","34","34.0"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35","6.35","","6.35","","9.52","9.52","9.52","9.52","","9.52","","","9.52","","6.40","6.35"]
["","Gas","","D.E.","mm","12.7","12.70","12.7","","12.70","","15.90","15.9","15.90","15.9","","15.90","","","15.90","","9.50","9.50"]
["","Drenaje","","","","VP20","VP20","VP20","","VP20","","VP20","VP20","VP20","VP20","","VP20","","","VP20","","VP20","VP20"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","BRC7GA53, BRC7GA56","BRC7F530W (panel blanco), BRC7GA56","BRC7GA53, BRC7GA56","","BRC7F530W (panel blanco), BRC7GA56","","BRC7F530W (panel blanco), BRC7GA56","BRC7GA53, BRC7GA56","BRC7F530W (panel blanco), BRC7GA56","BRC7GA53, BRC7GA56","","BRC7F530W (panel blanco), BRC7GA56","","","BRC7F530W (panel blanco), BRC7GA56","","BRC7GA53, BRC7GA56","BRC7F530W (panel blanco), BRC7GA56"]
["","Controlador remoto con cable","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","","1~","","1~","1~","1~","1~","","1~","","","1~","","1~","1~"]
["","Frecuencia","","","Hz","50","50/60","50","","50/60","","50/60","50","50/60","50","","50/60","","","50/60","","50","50/60"]
["","Tensión","","","V","220-240","220-240/220","220-240","","220-240/220","","220-240/220","220-240","220-240/220","220-240","","220-240/220","","","220-240/220","","220-240","220-240/220"]
["Accesorios estándar","Thermal insulation tube","","","","2","2","2","","2","","2","","","","","2","","","2","","2","2"]
["","Resin bushing","","","","1","1","1","","1","","1","","","","","1","","","1","","1","1"]
["","Wiring fixture","","","","2","2","2","","2","","2","","","","","2","","","2","","2","2"]
["","Hose band","","","","1","1","1","","1","","1","","","","","1","","","1","","1","1"]
["","Wire clamp material","","","","7","7","7","","7","","7","","","","","7","","","7","","7","7"]
["","Drain hose","","","","1","1","1","","1","","1","","","","","1","","","1","","1","1"]
["","Screws","","","","2","2","2","","2","","2","","","","","2","","","2","","2","2"]
["","Sealing pad (large)","","","","1","","1","","","","","","","","","","","","","","1"]
["","Sealing pad (small)","","","","1","","1","","","","","","","","","","","","","","1"]
["","Washer","","","","8","8","8","","8","","8","","","","","8","","","8","","8","8"]
["","General safety precautions","","","","","1","","","1","","1","","","","","1","","","1","","","1"]
["","Installation and operation manual","","","","","1","","","1","","1","","","","","1","","","1","","","1"]
["","Paper pattern for installation","","","","","1","","","1","","1","","","","","1","","","1","","","1"]
["","Sealing material","","","","","6","","","6","","6","","","","","6","","","6","","","6"]
["","Tubo de aislamiento térmico","","","","","","","","","","","2","2","2"]
["","Casquillo de resina","","","","","","","","","","","1","1","1"]
["","Montaje de sujeción del cableado","","","","","","","","","","","2","2","2"]
["","Abrazadera de tubo flexible","","","","","","","","","","","1","1","1"]
["","Material de la abrazadera para cables","","","","","","","","","","","7","7","7"]
["","Tubo flexible de drenaje","","","","","","","","","","","1","1","1"]
["","Tornillos","","","","","","","","","","","2","2","2"]
["","Almohadilla de sellado (grande)","","","","","","","","","","","1","","1"]
["","Almohadilla de sellado (pequeña)","","","","","","","","","","","1","","1"]
["","Arandela","","","","","","","","","","","8","8","8"]
["Notas","","","","","","","","","","","","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos.","","","","","","","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos."]
["Accesorios estándar","Precauciones generales de seguridad","","","","","","","","","","","","1"]
["","Manual de instalación y de uso","","","","","","","","","","","","1"]
["","Patrón impreso para la instalación","","","","","","","","","","","","1"]
["","Material de sellado","","","","","","","","","","","","6"]