{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Capacidad de refrigeración","Nom.","","kW","3.40"]
["Refrigeración de habitaciones","SEER","","","6.24"]
["","Consumo energético anual","","kWh/a","191"]
["","Capacidad","Pdesign","kW","3.40"]
["","Clase de eficiencia energética","","","A++"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Clase de eficiencia energética","","","A+"]
["","Consumo energético anual","","kWh/a","979"]
["Eficiencia nominal","Consumo energético anual","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A"]
["","","Calefacción","","A"]
["Capacidad de calefacción","Nom.","","kW","4.00"]
["Notas","","","","(1) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","(2) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(3) - Capacidades nom. de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","(4) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Capacidad de refrigeración","Nom.","","kW","","5.00","5.70"]
["Capacidad de calefacción","Nom.","","kW","","6.00","7.20"]
["Eficiencia nominal","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Consumo energético anual","","kWh","","780","867"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","B","A"]
["","","Calefacción","","","C","C"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","","A+","A+"]
["","Capacidad","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Consumo energético anual","","kWh/a","","295","328"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","","A","A"]
["","Capacidad","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Capacidad de calefacción Pdh a -10°","","kW","","3.85","4.08"]
["","Consumo energético anual","","kWh/a","","1578","1704"]