{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXS-L"]
[]
[]
[]
[]
["","","","","FHA50AVEB / RXS50L2V1B","FHA60AVEB / RXS60L2V1B"]
["Capacidad de refrigeración","Nom.","","kW","5.00","5.70"]
["Refrigeración de habitaciones","SEER","","","5.87","6.02"]
["","Consumo energético anual","","kWh/a","298","332"]
["","Capacidad","Pdesign","kW","5.00","5.70"]
["","Clase de eficiencia energética","","","A+","A+"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","4.35","4.71"]
["","SCOP/A","","","3.86","3.87"]
["","Clase de eficiencia energética","","","A","A"]
["","Consumo energético anual","","kWh/a","1,578","1,705"]
["Eficiencia nominal","EER","","","3.27","3.31"]
["","Consumo energético anual","","kWh","765","861"]
["","COP","","","3.35","3.32"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","A","A"]
["","","Calefacción","","C","C"]
["Capacidad de calefacción","Nom.","","kW","6.00","7.20"]
["Notas","","","","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m.","(1) - Capacidades nominales de refrigeración basadas en: temperatura interior: 27°CBS / 19°CBH; temperatura exterior: 35°CBS; tubería de refrigerante equivalente: 5m; diferencia de nivel: 0m."]
["","","","","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m.","(2) - Capacidades nominales de calefacción basadas en: temperatura interior 20°CBS; temperatura exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5 m; diferencia de nivel 0m."]
["","","","","(3) - Consulte la ilustración por separado para el rango de funcionamiento","(3) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","(4) - Consulte en el plano independiente con los datos eléctricos.","(4) - Consulte en el plano independiente con los datos eléctricos."]