{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B"]
["Rango de eficiencia energética","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","","","A+++ ~ D"]
["Refrigeración de habitaciones","SEER","","","","","","","","5.10","5.10","6.86","5.10","5.10","5.10","5.10"]
["","Consumo energético anual","","kWh/a","","","","","","467","467","347","467","652","652","652"]
["","Capacidad","Pdesign","kW","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Clase de eficiencia energética","","","","","","","","A","A","A++","A","A","A","A"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","","","","","","6.00","6.00","7.60","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","3.80","3.80","4.32","3.80","3.80","3.80","3.80"]
["","Clase de eficiencia energética","","","","","","","","A","A","A+","A","A","A","A"]
["","Consumo energético anual","","kWh/a","","","","","","2,211","2,211","2,463","2,211","4,164","4,164","4,164"]
["Notas","","","","","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","","","","","","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["Capacidad de refrigeración","Nom.","","kW","","","","","","","","6.80 (1)"]
["Eficiencia nominal","Annual energy consumption","","kWh","","","","","","","","890"]
["","EER","","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","","4.13 (3)"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","","","","","","A"]
["","","Calefacción","","","","","","","","","A"]
["Capacidad de calefacción","Nom.","","kW","","","","","","","","7.50 (2)"]
["Refrigeración de habitaciones","Clase de eficiencia energética","","","","","","","","","","","","","","","A"]
["","Capacidad","Pdesign","kW","","","","","","","","","","","","","12.00"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Consumo energético anual","","kWh/a","","","","","","","","","","","","","824"]
["Calefacción de habitaciones (clima medio)","Clase de eficiencia energética","","","","","","","","","","","","","","","A"]
["","Capacidad","Pdesign","kW","","","","","","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Capacidad de calefacción Pdh a -10°","","kW","","","","","","","","","","","","","11"]
["","Consumo energético anual","","kWh/a","","","","","","","","","","","","","4683"]