{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Nivel de presión sonora","Calefacción","Alto","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Medio","dBA","31","32","33","34"]
["","Refrigeración","Medio","dBA","34","35","35","36"]
["","","Bajo","dBA","31","32","33","34"]
["","","Alto","dBA","36","37","37","38"]
["Accesorios estándar","Tubo de aislamiento térmico","","","2","2","2","2"]
["","Material de la abrazadera para cables","","","7","7","7","7"]
["","Abrazadera de tubo flexible","","","1","1","1","1"]
["","Tubo flexible de drenaje","","","1","1","1","1"]
["","Arandela","","","8","8","8","8"]
["","Almohadilla de sellado (grande)","","","1","1","1","1"]
["","Almohadilla de sellado (pequeña)","","","1","1","1","1"]
["","Casquillo de resina","","","1","1","1","1"]
["","Tornillos","","","2","2","2","2"]
["","Montaje de sujeción del cableado","","","2","2","2","2"]
["Sistemas de control","Controlador remoto con cable","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Conexiones de tubería","Líquido","D.E.","mm","6.35","6.35","6.35","9.52"]
["","Gas","D.E.","mm","9.50","12.7","12.7","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20"]
["Nivel de potencia sonora","Refrigeración","","dBA","53","54","54","55"]
["Dimensiones","Unidad","Anchura","mm","960","960","1,270","1,270"]
["","","Profundidad","mm","690","690","690","690"]
["","","Altura","mm","235","235","235","235"]
["Carcasa","Material","","","Resina, metal laminado","Resina, metal laminado","Resina, metal laminado","Resina, metal laminado"]
["","Color","","","Blanco","Blanco","Blanco","Blanco"]
["Peso","Unidad","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frecuencia","","Hz","50","50","50","50"]
["","Tensión","","V","220-240","220-240","220-240","220-240"]
["Notas","","","","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos.","(1) - Consulte en el plano independiente con los datos eléctricos."]