{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B8 / RXS-F"]
[]
[]
[]
[]
["","","","","FHQ60BWV1B / RXS60F3V1B"]
["Capacidad de refrigeración","Mín.","","kW","1.7"]
["","Máx.","","kW","6.0"]
["","Nom.","","kW","5.7 (3)"]
["Conexiones de tubería","Liquid","OD","mm","6.35"]
["","Gas","D.E.","mm","12.7"]
["","Drain","OD","mm","VP20 (Diá. ext. 26, diá. int. 20)"]
["Eficiencia nominal","Annual energy consumption","","kWh","1,075"]
["","EER","","","2.65"]
["","COP","","","2.89"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","D"]
["","","Calefacción","","D"]
["Capacidad de calefacción","Nom.","","kW","7.2 (4)"]
["","Mín.","","kW","1.7"]
["","Máx.","","kW","8.0"]
["Notas","","","","(1) - Etiqueta de eficiencia energética: escala desde A (más eficiente) a G (menos eficiente)"]
["","","","","(2) - Consumo anual de energía: basado en un promedio de utilización de 500 horas de uso al año a plena carga (condiciones nominales)"]
["","","","","(3) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS, 24°CBH; longitud de tubería equivalente 5m"]
["","","","","(4) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m"]
["","","","","(5) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]