{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":23,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ100CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ125CBVEB / RZQG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Capacidad de refrigeración","Nom.","","kW","","","","","6.8","","9.5","","","","","","","12.0","","","","","13.4"]
["Refrigeración de habitaciones","SEER","","","6.95","5.10","5.10","5.10","6.86","5.10","6.11","6.11","5.10","5.10","5.10","5.10","5.10","6.01","5.10","6.01","5.10","5.10"]
["","Consumo energético anual","","kWh/a","343","467","467","467","347","652","545","545","652","652","652","652","824","699","824","699","824","824"]
["","Capacidad","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Clase de eficiencia energética","","","A++","B","B","B","A++","B","A++","A++","B","B","B","B","B","A+","B","A+","B","B"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","7.60","6.00","6.00","6.00","7.60","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","14.13","12.71","14.13","12.71","12.71"]
["","SCOP/A","","","4.32","3.80","3.80","3.80","4.32","3.80","4.61","4.61","3.80","3.80","3.80","3.80","3.80","4.23","3.80","4.23","3.80","3.80"]
["","Clase de eficiencia energética","","","A+","A","A","A","A+","A","A++","A++","A","A","A","A","A","A+","A","A+","A","A"]
["","Consumo energético anual","","kWh/a","2,463","2,211","2,211","2,211","2,463","4,164","3,432","3,432","4,164","4,164","4,164","4,164","4,683","4,677","4,683","4,677","4,683","4,683"]
["Eficiencia nominal","Annual energy consumption","","kWh","","","","","890","","1,245","","","","","","","1,790","","","","","2,025"]
["","EER","","","","","","","3.82","","3.81","","","","","","","3.35","","","","","3.31"]
["","COP","","","","","","","4.13","","4.15","","","","","","","3.89","","","","","3.63"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","","","","","A","","A","","","","","","","A","","","","","A"]
["","","Calefacción","","","","","","A","","A","","","","","","","A","","","","","A"]
["Capacidad de calefacción","Nom.","","kW","","","","","7.5","","10.8","","","","","","","13.5","","","","","15.5"]
["Notas","","","","","","","","(1) - Consumo anual de energía de acuerdo con la Directiva de etiquetado energético 2002/31/EC","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","","","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","","","","","(2) - SEER y SCOP conforme a EN 14825","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","","","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal","","","","","(2) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]